What we need is the .DMO configuration file for each DX-9100 system. If the customer doesn’t have that available you can recreate it by uploading and saving the configuration with the GX9100 utility. It is available as part of the M-Tools package that you can purchase through distribution.